|  |  |  |  |
| --- | --- | --- | --- |
| **PLANT DETAILS** | | | |
| Plant Owner: | Address: | | Ph: |
| Plant Make: | Plant Model: | Plant Serial No: | Hours / KM’s: |
| Roads Reg No: | Reg Expiry: | Project Registration No: | Project Asset No: |
| Last Service Date / Hrs: | Next service Date / Hrs: |  |  |
| **MINIMUM REQUIREMENTS (If the minimum requirements are not met, a plant sticker will not be issued and the item of plant is not to commence work)** | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Verify** | **Check** | **Requirement** | **Verify** | **Check** | **Requirement** |
|  |  | Operator and Maintenance Manual available |  |  | Plant Hazard Assessment Sighted & Current (within 2 yrs): |
|  |  | Logbook / Service Records (checked ok): |  |  | Plant Hazard Assessment Inspection Date: / / |
|  |  | Audible Alarm and other Warning Devices fitted, operable and suitable for site conditions |  |  | Daily Prestart Inspection Checklist is available for use. |
|  |  | Fire Extinguisher Fitted and charged |  |  |  |

|  |  |  |
| --- | --- | --- |
| **Verify** | **Check** | **Cabin** |
|  |  | Cleanliness |
|  |  | Door operational |
|  |  | Deadman Pedal /Switch operational |
|  |  | Handrails and ladders fitted and secure |
|  |  | Seat – adjustments operational secure |
|  |  | Seat belt fitted and in good working order |
|  |  | Instruments operational & labeled |
|  |  | Levers / Controls Operational |
|  |  | Pedals in good condition |
|  |  | Air conditioning operational |
|  |  | Wipers / Washers operational |
|  |  | Rear View Mirrors |
|  |  | ROPs and FOPs Canopy to meet AS 2294 |
|  |  | Windows not damaged |
|  |  | SWL / Crane Chart |
|  |  | Warning devices and other lights (flashing, head, tail, etc) are appropriate for the environment in which plant is being used. (check environment noise criteria particularly if working out of hours) |
|  |  | Warning Signs - Seat belt must be worn |
|  |  | Warning Signs - Dial Before You Dig |
|  |  | Warning Signs - Danger – Beware Overhead Wires & Underground Services |
| **Verify** | **Check** | **Hydraulics** |
|  |  | Rams |
|  |  | Hoses |
|  |  | Connections (check for excessive wear, leaks and creep) |
|  |  | Crane valves / Hose Burst Protection if used for Lifting or Maximum1000KG SWL located on loader frame or Jib |

|  |  |  |
| --- | --- | --- |
| **Verify** | **Check** | **Environmental** |
|  |  | Clean, free of organic materials (mud, dirt, weeds or seeds) prior to arrival |
|  |  | Engine baffling or noise reduction equipment fitted as per manufacturers specifications |
|  |  | Smoke from internal combustion engines should not be visible for more than ten seconds |

|  |  |  |
| --- | --- | --- |
| **Verify** | **Check** | **Engine** |
|  |  | Engine Guarding |
|  |  | Exhaust Guarding |
|  |  | Fluid levels |
|  |  | Water Leaks/ levels checked |
|  |  | Radiator Hose & Clamps |
|  |  | Radiator Core Condition |
|  |  | Vee Belt Condition |
|  |  | Fan Hub Bearings |
|  |  | Oil Leaks /levels checked |
|  |  | Air Intake Hoses & Clamps |
|  |  | Air Cleaner |
|  |  | Mountings |
|  |  | Battery Condition |
| **Verify** | **Check** | **Running Controls** |
|  |  | Tyres / Wheels undamaged |
|  |  | Brake operational |
|  |  | Park brake is operational |
| **Verify** | **Check** | **Steering** |
|  |  | Steering Linkages / Rams |
|  |  | Connectors |
|  |  | Safety Pins |
|  |  | Pivots |
|  |  | Articulation bearings and retainers |
|  |  | Artic safety lock |

**Instructions: Verify Box to be ticked by Owner / Supplier / Operator prior to arrival onsite. Check Box to be ticked after visual inspection by the project**



|  |  |  |  |
| --- | --- | --- | --- |
| **TYRES – Record Tread Depth (if required)** | | | |
| **POS 1 (LF)** | **\_\_\_\_mm** | **POS 2 (RF)** | **\_\_\_\_mm** |
| **POS 3 (LR)** | **\_\_\_\_mm** | **POS 4 (RR)** | **\_\_\_\_mm** |

|  |  |
| --- | --- |
| **PLANT OWNER / OCCUPIER** | **PLANT VERIFIER** |
| I certify that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications | I certify that I have verified that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications |
| Name: Signature: Date: | Name: Signature: Date: |