|  |  |  |  |
| --- | --- | --- | --- |
| **PLANT DETAILS** | | | |
| Plant Owner: | Address: | | Ph: |
| Plant Make: | Plant Model: | Plant Serial No: | Hours / KM’s: |
| Roads Reg No: | Reg Expiry: | Project Registration No: | Project Asset No: |
| Last Service Date / Hrs: | Next service Date / Hrs: |  |  |
| **MINIMUM REQUIREMENTS** (If the minimum requirements are not met, a plant sticker will not be issued and the item of plant is not to commence work) | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Verify** | **Check** | **Requirement** | **Verify** | **Check** | **Requirement** |
|  |  | Operator and Maintenance Manual available |  |  | Plant Hazard Assessment Sighted & Current (within 2 yrs): |
|  |  | Logbook / Service Records (checked ok): |  |  | Plant Hazard Assessment Inspection Date: / / |
|  |  | Audible Alarm and other Warning Devices fitted, operable and suitable for site conditions |  |  | Daily Prestart Inspection Checklist is available for use. |
|  |  | Fire Extinguisher Fitted and charged |  |  |  |

|  |
| --- |
| **Instructions: Verify Box** to be ticked by Owner / Supplier / Operator prior to arrival onsite. **Check Box** to be ticked after visual inspection by the project |
| |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Cabin** | |  |  | Cleanliness | |  |  | Door operational | |  |  | Grab rails and ladders fitted and secure | |  |  | Seat – adjustments operational secure | |  |  | Instruments operational & labelled | |  |  | Seat Belts fitted | |  |  | Levers / Controls Operational | |  |  | Pedals in good condition | |  |  | Air conditioning operational | |  |  | Wipers / Washers operational | |  |  | Seat belt fitted and in good working order | |  |  | UHF Radio Fitted (If not fitted, has a hand held radio been supplied) | |  |  | First Aid Kit available | |  |  | Warning devices and other lights (flashing, head, tail, etc) are appropriate for the environment in which plant is being used. (check environment noise criteria particularly if working out of hours) | |  |  | Rear View Mirrors | | **Verify** | **Check** | **Tray** | |  |  | Access ladder clean and undamaged to tipper | |  |  | Tail gate locks operational | |  |  | Tarps provided | | **Verify** | **Check** | **Tipper Body** | |  |  | Temporary propping stand fitted | |  |  | Hand grabs and ladders fitted and secure |  |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Environmental** | |  |  | Clean, free of organic materials (mud, dirt, weeds or seeds) prior to arrival | |  |  | Engine baffling or noise reduction equipment fitted as per manufacturers specifications | |  |  | Smoke from internal combustion engines should not be visible for more than ten seconds |  |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Steering** | |  |  | Unions | |  |  | Pivots | |  |  | Connecting Rods | |  |  | Steering Linkages | | **Verify** | **Check** | **Hydraulics** | |  |  | Rams | |  |  | Hoses / Connectors | |  |  | Hydraulics levels checked | |  |  | Pins / Mounting | |  |  | (check for excessive  wear, leaks and creep) | |  |  | Hoist control from cabin | |  |  | Tail gate control from cabin | | **Verify** | **Check** | **Engine** | |  |  | Engine Mountings | |  |  | Engine Guarding | |  |  | Exhaust Guarding | |  |  | Oil Leaks/levels checked | |  |  | Coolant Leaks/levels checked | |  |  | Coolant System | |  |  | Vee Belt Condition | |  |  | Air Cleaner System | |  |  | Battery Condition / Mounting |  |  |  |  |  | | --- | --- | --- | --- | | TYRES – Record Tread Depth (*if required)* | | | | | POS 1 (LF) | \_\_\_\_mm | POS 2 (RF) | \_\_\_\_mm | | POS 3 (LF2) | \_\_\_\_mm | POS 4 (RF2) | \_\_\_\_mm | | POS 5 (LR3) | \_\_\_\_mm | POS 6 (RR3) | \_\_\_\_mm | |
|
|
|
|
|
|
|
|
|
|
|
|
|
|
| |  |  | | --- | --- | | **PLANT OWNER / OCCUPIER** | **PLANT VERIFIER** | | I certify that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications | I certify that I have verified that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications | | Name: Signature: Date: | Name: Signature: Date: | |