|  |  |  |  |
| --- | --- | --- | --- |
| **PLANT DETAILS** | | | |
| Plant Owner: | Address: | | Ph: |
| Plant Make: | Plant Model: | Plant Serial No: | Hours / KM’s: |
| Roads Reg No: | Reg Expiry: | Project Registration No: | Project Asset No: |
| Last Service Date / Hrs: | Next service Date / Hrs: |  |  |
| **MINIMUM REQUIREMENTS** (If the minimum requirements are not met, a plant sticker will not be issued and the item of plant is not to commence work) | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | **Verify** | **Check** | **Requirement** | **Verify** | **Check** | **Requirement** | |  |  | Operator and Maintenance Manual available |  |  | Plant Hazard Assessment Sighted & Current (within 2 yrs): | |  |  | Logbook / Service Records (checked ok): |  |  | Plant Hazard Assessment Inspection Date: / / | |  |  | Audible Alarm and other Warning Devices fitted, operable and suitable for site conditions |  |  | Daily Prestart Inspection Checklist is available for use. | |  |  | Fire Extinguisher Fitted and charged |  |  |  | | | | |

|  |
| --- |
| **Instructions: Verify Box** to be ticked by Owner / Supplier / Operator prior to arrival onsite. **Check Box** to be ticked after visual inspection by the project |
| |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Cabin** | |  |  | Cleanliness | |  |  | Deadman Pedal /Switch operational | |  |  | Handrails fitted and secure | |  |  | Seat – adjustments operational secure | |  |  | Description: http://renaissanceronin.files.wordpress.com/2009/11/tractor_3000.jpgSeat belt fitted and in good working order | |  |  | ROPs and FOPs (If using a bucket) Canopy to meet AS 2294 | |  |  | Instruments operational & labelled | |  |  | UHF Radio Fitted (If not fitted, has a hand held radio been supplied if required) | |  |  | Warning devices and other lights (flashing, head, tail, etc) are appropriate for the environment in which plant is being used. (check environment noise criteria particularly if working out of hours) | |  |  | Levers / Controls Operational | |  |  | Pedals in good condition | |  |  | Air conditioning operational (if fitted) | |  |  | Wipers / Washers operational (if fitted) | |  |  | Rear View Mirrors | |  |  | Windows not damaged if fitted | |  |  | Warning Signs - **Seat belt must be worn** | |  |  | Warning Signs - **Dial Before You Dig** | | **Verify** | **Check** | **Running Controls** | |  |  | Tyres / Wheels / undamaged | |  |  | Brake operational | |  |  | Park brake is operational |  |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Environmental** | |  |  | Clean, free of organic materials (mud, dirt, weeds or seeds) prior to arrival | |  |  | Engine baffling or noise reduction equipment fitted as per manufacturers specifications | |  |  | Smoke from internal combustion engines should not be visible for more than ten seconds |  |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Steering** | |  |  | Unions | |  |  | Pivots | |  |  | Connecting Rods | |  |  | Steering Linkages / Rams | | **Verify** | **Check** | **Hydraulics System** | |  |  | Rams | |  |  | Hoses / Connectors | |  |  | Pins / Mounting | |  |  | (check for excessive wear, leaks and creep) | | **Verify** | **Check** | **Engine** | |  |  | Engine Mountings | |  |  | Engine Guarding | |  |  | Exhaust Guarding | |  |  | Oil Leaks/check levels | |  |  | Coolant Leaks/check levels | |  |  | Coolant System | |  |  | Vee Belt Condition | |  |  | Air Cleaner System | |  |  | Battery Condition / Mounting | | **Verify** | **Check** | **Attachments** | |  |  | Quick hitch, 3 point linkage | |  |  | Front end loader |  |  |  |  |  | | --- | --- | --- | --- | | TYRES – Record Tread Depth (if required) | | | | | POS 1 (LF) | \_\_\_\_mm | POS 2 (RF) | \_\_\_\_mm | | POS 3 (LR) | \_\_\_\_mm | POS 4 (RR) | \_\_\_\_mm | |
|
|
|
|
|
|
|
|
|
|
|
|
|
|
|
|  |
| |  |  | | --- | --- | | **PLANT OWNER / OCCUPIER** | **PLANT VERIFIER** | | I certify that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications | I certify that I have verified that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications | | Name: Signature: Date: | Name: Signature: Date: | |