|  |  |  |  |
| --- | --- | --- | --- |
| **PLANT DETAILS** | | | |
| Plant Owner: | Address: | | Ph: |
| Plant Make: | Plant Model: | Plant Serial No: | Hours / KM’s: |
| Roads Reg No: | Reg Expiry: | Project Registration No: | Project Asset No: |
| Last Service Date / Hrs: | Next service Date / Hrs: |  |  |
| **MINIMUM REQUIREMENTS** (If the minimum requirements are not met, a plant sticker will not be issued and the item of plant is not to commence work) | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Verify** | **Check** | **Requirement** | **Verify** | **Check** | **Requirement** |
|  |  | Operator and Maintenance Manual available |  |  | Plant Hazard Assessment Sighted & Current (within 2 yrs): |
|  |  | Logbook / Service Records (checked ok): |  |  | Plant Hazard Assessment Inspection Date: / / |
|  |  | Audible Alarm and other Warning Devices fitted, operable and suitable for site conditions |  |  | Daily Prestart Inspection Checklist is available for use. |
|  |  | Fire Extinguisher Fitted and charged |  |  |  |

|  |
| --- |
| Instructions: Verify Box to be ticked by Owner / Supplier / Operator prior to arrival onsite. **Check Box** to be ticked after visual inspection by the project |
| |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Cabin** | |  |  | Cleanliness | |  |  | Handrails and ladders fitted and secure | |  |  | Seat – adjustments operational secure | |  |  | Seat belt fitted and in good working order | |  |  | UHF Radio Fitted (If not fitted, has a hand held radio been supplied) | |  |  | First Aid Kit, triangle and road reflectors available | |  |  | Warning devices and other lights (flashing, head, tail, etc) are appropriate for the environment in which plant is being used. (check environment noise criteria particularly if working out of hours) | |  |  | Instruments operational & labelled | |  |  | Levers / Controls Operational | |  |  | Pedals in good condition | |  |  | Air conditioning operational | |  |  | Wipers / Washers operational | |  |  | Description: http://niftylift.buaconsulting.com/images/topimage1.pngRear View Mirrors | | **Verify** | **Check** | Windows not damaged | |  |  | Rams | |  |  | Hoses / Connectors | |  |  | Pins / Mounting | |  |  | (check for excessive wear, leaks and creep) | | **Verify** | **Check** | **Running Gear** | |  |  | Tyres / Wheels undamaged | |  |  | Hand brake is operational | |  |  | Brake operational |  |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Lifting Mechanism** | |  |  | Pivots | |  |  | Connecting Rods | |  |  | Safety Pins (No excessive wear) | | **Verify** | **Check** | **Operation** | |  |  | Ground-level operating controls | |  |  | Levers / controls guarded against in advertent operation | |  |  | Deadman Switch operational | | **Verify** | **Check** | **Engine** | |  |  | Engine Guarding | |  |  | Exhaust (if applicable) | |  |  | Fluid levels/checked | | **Verify** | **Check** | **Warning Signs** | |  |  | Warning Signs - **Danger – Beware Overhead Wires** | |  |  | Limits of internal & external use | |  |  | Wind Speed Capability | |  |  | Safe Working Load | | **Verify** | **Check** | **Outriggers** | |  |  | Function test | |  |  | Out rigger pads available |  |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Environmental** | |  |  | Clean, free of organic materials (mud, dirt, weeds or seeds) prior to arrival | |  |  | Engine baffling or noise reduction equipment fitted as per manufacturers specifications | |  |  | Smoke from internal combustion engines should not be visible for more than ten seconds | | **Verify** | **Check** | **Basket** | |  |  | Cleanliness | |  |  | Operator restraint ( harness and lanyard) available | |  |  | Self-Closing gate operational | |  |  | Estop switch in basket and on the base unit functioning | |  |  | Handrails are fitted and secured | |  |  | Anchor points are in place and not damaged | |  |  | Guards on operators control panel to prevent hand being trapped | |  |  | Horn and alarms operable (raise /lower, out of level, motion alarms) | |  |  | Warning devices and other lights (flashing, head, tail, indicators) | |  |  | Safety harness and lanyard |  |  |  |  |  | | --- | --- | --- | --- | | **TYRES – Record Tread Depth (*if required)*** | | | | | POS 1 (LF) | \_\_\_\_mm | POS 2 (RF) | \_\_\_\_mm | | POS 3 (LF2) | \_\_\_\_mm | POS 4 (RF2) | \_\_\_\_mm | | POS 5 (LR3) | \_\_\_\_mm | POS 6 (RR3) | \_\_\_\_mm | |
|
|
|
|
|
|
|
|
|
|
|
|
|
|

|  |  |
| --- | --- |
| **PLANT OWNER / OCCUPIER** | **PLANT VERIFIER** |
| I certify that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications | I certify that I have verified that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications |
| Name: Signature: Date: | Name: Signature: Date: |