|  |  |  |  |
| --- | --- | --- | --- |
| **PLANT DETAILS** | | | |
| Plant Owner: | Address: | | Ph: |
| Plant Make: | Plant Model: | Plant Serial No: | Hours / KM’s: |
| Roads Reg No: | Reg Expiry: | Project Registration No: | Project Asset No: |
| Last Service Date / Hrs: | Next service Date / Hrs: |  |  |
| **MINIMUM REQUIREMENTS** (If the minimum requirements are not met, a plant sticker will not be issued and the item of plant is not to commence work) | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Verify** | **Check** | **Requirement** | **Verify** | **Check** | **Requirement** |
|  |  | Operator and Maintenance Manual available |  |  | Plant Hazard Assessment Sighted & Current (within 2 yrs): |
|  |  | Logbook / Service Records (checked ok): |  |  | Plant Hazard Assessment Inspection Date: / / |

|  |
| --- |
| **Instructions:** Verify Box to be ticked by Owner / Supplier / Operator prior to arrival onsite. Check Box to be ticked after visual inspection by the project. |
| |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Rock Saw** | |  |  | Rock saw is sized / rated for the excavator size | |  |  | Hydraulic hoses & fittings are free of damage | |  |  | Hydraulic fittings match that of the excavator it is to be used on | |  |  | No leaks from rock saw | |  |  | Structure free from cracks and damage | |  |  | Blade mounting bolts fitted and tight | |  |  | Condition of the blade, - No more than 3 teeth missing, Wear on blade and teeth | |  |  | All safety guards secure and in good condition | |  |  | Water spray Available | |  |  | Case drain lines fitted to excavator | |  |  | Correct direction of rotation | |  |  | Machine hydraulics (flow and pressure) match requirements of the saw. | |  |  | Approval from manufacturer to use rock saw on machinery |  |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Hitch** | |  |  | Hitch matches that of the excavator | |  |  | Hitch is designed for use with rock saw attachment | |  |  | Maintained and in good working order | |  |  | Quick hitch safety pins and locks available and in good working order | |  |  | Marked with the following Manufacturer's name, make, model and serial number | |  |  | Hitch pins are fitted with retainer bolts | |  |  | Pins / bosses not worn or cracked |  |  |  |  | | --- | --- | --- | | **Verify** | **Check** | **Environmental** | |  |  | Clean, free of organic materials (mud, dirt, weeds or seeds) prior to arrival | |  |  | Engine baffling or noise reduction equipment fitted as per manufacturers specifications | |
|
|
|
|
|
|
|
|
|
|
| |  |  | | --- | --- | | **PLANT OWNER / OCCUPIER** | **PLANT VERIFIER** | | I certify that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications | I certify that I have verified that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications | | Name: Signature: Date: | Name: Signature: Date: | |