|  |
| --- |
| **PLANT DETAILS** |
| Plant Owner: | Address: | Ph: |
| Plant Make: | Plant Model: | Plant Serial No: | Hours / KM’s: |
| Roads Reg No: | Reg Expiry: | Project Registration No: | Project Asset No: |
| Last Service Date / Hrs: | Next service Date / Hrs: |  |  |
| **MINIMUM REQUIREMENTS** (If the minimum requirements are not met, a plant sticker will not be issued and the item of plant is not to commence work) |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Verify** | **Check** | **Requirement** | **Verify** | **Check** | **Requirement** |
|  |  | Operator and Maintenance Manual available |  |  | Plant Hazard Assessment Sighted & Current (within 2 yrs): |
|  |  | Logbook / Service Records (checked ok): |  |  | Plant Hazard Assessment Inspection Date: / /  |

|  |
| --- |
| **Instructions:** Verify Box to be ticked by Owner / Supplier / Operator prior to arrival onsite. Check Box to be ticked after visual inspection by the project. |
|

|  |  |  |
| --- | --- | --- |
| **Verify** | **Check** | **Twin Header** |
|  |  | Twin Header is sized / rated for the excavator size |
|  |  | Hydraulic hoses & fittings are free of damage |
|  |  | Hydraulic fittings match that of the excavator it is to be used on |
|  |  | No leaks from Twin Header |
|  |  | Housing free from cracks and damage |
|  |  | Condition of pick’s |
|  |  | Condition of pick blocks |
|  |  | Picks clear centre housing |
|  |  | Cutter drum retaining bolts fitted and tight |
|  |  | Oil level in gearbox |
|  |  | Correct rotation direction known |
|  |  | Maximum flow and pressure the header can handle is not exceeded on the output side of the excavator’s hydraulics. |
|  |  | Case drain line available on excavator |

|  |  |  |
| --- | --- | --- |
| **Verify** | **Check** | **Hitch** |
|  |  | Hitch matches that of the excavator |
|  |  | Hitch is designed for use with Twin Header attachment |
|  |  | Maintained and in good working order |
|  |  | Safety pins and locks available, in good working order |
|  |  | Marked with the following Manufacturer's name, make, model and serial number |
|  |  | Hitch pins are fitted with retainer bolts |
|  |  | Pins / bosses not worn or cracked |
|  |  | Mounting cup bolts fitted and tight |
| **Verify** | **Check** | **Environmental** |
|  |  | Clean, free of organic materials (mud, dirt, weeds or seeds) prior to arrival |
|  |  | Engine baffling or noise reduction equipment fitted as per manufacturers specifications |

 |
|
|
|
|
|
|
|
|
|
|
|
|
|
|

|  |  |
| --- | --- |
| **PLANT OWNER / OCCUPIER** | **PLANT VERIFIER** |
| I certify that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications | I certify that I have verified that the described plant has met the inspection criteria stipulated within this checklist and is being serviced and maintained in accordance with the manufacturer’s specifications |
| Name: Signature: Date: | Name: Signature: Date: |